*************************** START ****************************

START TIME: 202309261737

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fc4608
mac h: 0x96a0b7
crc_cal: 150
crc_read: 150
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.4 seconds (effective 395.6 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 599.4 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 9.7 seconds (effective 780.5 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 12 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309271102

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fc4608
mac h: 0x96a0b7
crc_cal: 150
crc_read: 150
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 286.0 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 323.4 kbit/s)...

Hash of data verified.
Wrote 952304 bytes (617163 compressed) at 0x00010000 in 9.9 seconds (effective 770.5 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309271107

CONNECT BAUD: 115200
serial port open error
COM:COM17
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309271107

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202309271107

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fc4608
mac h: 0x96a0b7
crc_cal: 150
crc_read: 150
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 284.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 323.4 kbit/s)...

Hash of data verified.
Wrote 952304 bytes (617163 compressed) at 0x00010000 in 9.8 seconds (effective 774.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 40 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309271121

CONNECT BAUD: 115200
serial port open error
COM:COM17
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309271121

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fc4608
mac h: 0x96a0b7
crc_cal: 150
crc_read: 150
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 285.6 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 327.7 kbit/s)...

Hash of data verified.
Wrote 951936 bytes (616885 compressed) at 0x00010000 in 9.8 seconds (effective 776.2 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309271127

CONNECT BAUD: 115200
serial port open error
COM:COM17
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309271127

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fc4608
mac h: 0x96a0b7
crc_cal: 150
crc_read: 150
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 283.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 327.7 kbit/s)...

Hash of data verified.
Wrote 951936 bytes (616885 compressed) at 0x00010000 in 9.8 seconds (effective 780.9 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 41 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309271133

CONNECT BAUD: 115200
serial port open error
COM:COM17
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309271133

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fc4608
mac h: 0x96a0b7
crc_cal: 150
crc_read: 150
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 285.6 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 327.7 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 9.7 seconds (effective 778.6 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309271203

CONNECT BAUD: 115200
serial port open error
COM:COM17
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309271203

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fc4608
mac h: 0x96a0b7
crc_cal: 150
crc_read: 150
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 284.0 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 327.7 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 9.7 seconds (effective 780.0 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 39 s

Download result: PASS

*************************** END ****************************



