*************************** START ****************************

START TIME: 202309261525

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.4 seconds (effective 367.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 558.5 kbit/s)...

Hash of data verified.
Wrote 951936 bytes (616885 compressed) at 0x00010000 in 11.1 seconds (effective 685.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 23 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261529

CONNECT BAUD: 115200
serial port open error
COM:COM15
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309261529

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.6 seconds (effective 273.2 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 307.2 kbit/s)...

Hash of data verified.
Wrote 951936 bytes (616885 compressed) at 0x00010000 in 10.9 seconds (effective 701.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 34 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261532

CONNECT BAUD: 115200
serial port open error
COM:COM15
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309261533

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.6 seconds (effective 273.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 307.2 kbit/s)...

Hash of data verified.
Wrote 951936 bytes (616885 compressed) at 0x00010000 in 10.9 seconds (effective 700.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261535

CONNECT BAUD: 115200
serial port open error
COM:COM15
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309261535

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016

com closed
Use time: 40 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261536

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202309261536

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016

com closed
Use time: 29 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261536

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016

com closed
Use time: 19 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261537

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.4 seconds (effective 372.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 558.6 kbit/s)...

Hash of data verified.
Wrote 951936 bytes (616885 compressed) at 0x00010000 in 11.0 seconds (effective 691.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261547

CONNECT BAUD: 115200
serial port open error
COM:COM15
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309261547

CONNECT BAUD: 115200
serial port open error
COM:COM15
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309261547

CONNECT BAUD: 115200
serial port open error
COM:COM15
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309261547

CONNECT BAUD: 115200
serial port open error
COM:COM15
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309261548

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016

com closed
Use time: 80 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261549

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.4 seconds (effective 369.7 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 571.5 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 11.0 seconds (effective 691.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261551

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.6 seconds (effective 272.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 307.2 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 10.8 seconds (effective 699.3 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 22 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261648

CONNECT BAUD: 115200
serial port open error
COM:COM15
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309261648

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.6 seconds (effective 269.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 307.2 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 10.8 seconds (effective 701.2 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 72 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261652

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.6 seconds (effective 269.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 311.1 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 10.8 seconds (effective 699.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261655

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202309261656

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.6 seconds (effective 268.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 311.1 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 10.8 seconds (effective 702.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 36 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261716

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.6 seconds (effective 270.2 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 307.2 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 10.8 seconds (effective 701.6 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261716

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202309261717

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202309261718

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.6 seconds (effective 273.2 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 311.1 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 10.8 seconds (effective 700.2 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 36 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261724

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.6 seconds (effective 269.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 311.1 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 10.8 seconds (effective 699.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309271903

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fcf288
mac h: 0x23a0b7
crc_cal: 35
crc_read: 35
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.6 seconds (effective 263.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 296.1 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 10.8 seconds (effective 700.0 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



