*************************** START ****************************

START TIME: 202310241119

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x93dfe1f4
mac h: 0xf4417
crc_cal: 15
crc_read: 15
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 281.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 323.1 kbit/s)...

Hash of data verified.*************************** START ****************************

START TIME: 202310241120

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x93dfe1f4
mac h: 0xf4417
crc_cal: 15
crc_read: 15
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 281.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 323.4 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 9.8 seconds (effective 776.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 27 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202310241131

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset state: ESP_DL_STOP
