*************************** START ****************************

START TIME: 202309071026

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 288.1 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 329.9 kbit/s)...

Hash of data verified.
Wrote 945888 bytes (613603 compressed) at 0x00010000 in 9.9 seconds (effective 763.6 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 36 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309071840

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016

com closed
Use time: 21 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309081748

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016

com closed
Use time: 8 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309081749

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.4 seconds (effective 400.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 614.4 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 9.7 seconds (effective 781.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 12 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309081828

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 289.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 332.1 kbit/s)...

Hash of data verified.
Wrote 951936 bytes (616885 compressed) at 0x00010000 in 10.0 seconds (effective 765.4 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 28 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309111605

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 288.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 332.1 kbit/s)...

Hash of data verified.
Wrote 951936 bytes (616885 compressed) at 0x00010000 in 9.9 seconds (effective 765.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 34 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309111609

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 288.9 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 336.7 kbit/s)...

Hash of data verified.
Wrote 951984 bytes (617009 compressed) at 0x00010000 in 9.9 seconds (effective 768.6 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 24 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309111614

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202309111614

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016

com closed
Use time: 27 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309111615

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.4 seconds (effective 400.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 630.1 kbit/s)...

Hash of data verified.*************************** START ****************************

START TIME: 202309111615

CONNECT BAUD: 115200
serial port open error
COM:COM18
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202309111615

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 292.2 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 336.7 kbit/s)...

Hash of data verified.
Wrote 951984 bytes (617009 compressed) at 0x00010000 in 9.7 seconds (effective 785.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 25 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309111616

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 292.2 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 336.7 kbit/s)...

Hash of data verified.
Wrote 951984 bytes (617009 compressed) at 0x00010000 in 9.9 seconds (effective 768.5 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 19 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261352

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016

com closed
Use time: 85 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261353

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016

set STOP FLG: Truecom closed
Use time: 15 s

Download result: PASS

*************************** END ****************************



set state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202309261355

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016

com closed
Use time: 15 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261355

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202309261356

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.4 seconds (effective 396.7 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 614.5 kbit/s)...

Hash of data verified.
Wrote 951936 bytes (616885 compressed) at 0x00010000 in 9.7 seconds (effective 787.0 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 13 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261400

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset state: ESP_DL_STOP
*************************** START ****************************

START TIME: 202309261400

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016

com closed
Use time: 1480 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261426

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.4 seconds (effective 396.5 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 571.5 kbit/s)...

Hash of data verified.
Wrote 952304 bytes (617163 compressed) at 0x00010000 in 9.7 seconds (effective 785.9 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 12 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202309261520

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x65fd8df8
mac h: 0xdea0b7
crc_cal: 222
crc_read: 222
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 289.4 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 327.7 kbit/s)...

Hash of data verified.
Wrote 951936 bytes (616885 compressed) at 0x00010000 in 9.8 seconds (effective 781.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 19 s

Download result: PASS

*************************** END ****************************



