*************************** START ****************************

START TIME: 202310241027

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x93dfff50
mac h: 0xf14417
crc_cal: 241
crc_read: 241
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016

com closed
Use time: 14 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202310241027

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x93dfff50
mac h: 0xf14417
crc_cal: 241
crc_read: 241
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.4 seconds (effective 407.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 630.1 kbit/s)...

Hash of data verified.*************************** START ****************************

START TIME: 202310241030

CONNECT BAUD: 115200
serial port open error
COM:COM30
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
*************************** START ****************************

START TIME: 202310241034

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0x93dfff50
mac h: 0xf14417
crc_cal: 241
crc_read: 241
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 18992 bytes (13112 compressed) at 0x00001000 in 0.5 seconds (effective 298.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.1 seconds (effective 360.6 kbit/s)...

Hash of data verified.
Wrote 946336 bytes (613774 compressed) at 0x00010000 in 9.3 seconds (effective 812.1 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 53 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202310241037

CONNECT BAUD: 115200
serial port open error
COM:COM30
baud:115200
SERIAL PORT OPEN ERROR
set state: ESP_DL_CONNECT_ERROR
